Jump to main content

# 13.8.2 RT PolarFire Licensing and Device/Package Combination Matrix

(Ask a Question)

Libero SoC v2021.1 introduces Preliminary timing and power support for RT PolarFire devices.

Table 13-6.RT PolarFire Licensing and Device/Package Combinations
(T/TL/TS/TLS), Speed Grade, Temperature | Part Number | Libero Licensing | Libero Timing/Power | Programming
--- | --- | --- | --- | ---
Eval | Silver | Gold | Platinum
T, STD, MIL, 1.0/1.05V | RTPF500T-CG1509M | Yes | — | — | Yes | Preliminary | Yes
T, -1, MIL, 1.0/1.05V | RTPF500T-1CG1509M | Yes | — | — | Yes | Preliminary | Yes
TS, STD, MIL, 1.0/1.05V | RTPF500TS-CG1509M | Yes | — | — | Yes | Preliminary | Yes
TS, -1, MIL, 1.0/1.05V | RTPF500TS-1CG1509M | Yes | — | — | Yes | Preliminary | Yes
TL, STD, MIL, 1.0/1.05V | RTPF500TL-CG1509M | Yes | — | — | Yes | Preliminary | Yes
TLS, STD, MIL, 1.0/1.05V | RTPF500TLS-CG1509M | Yes | — | — | Yes | Preliminary | Yes

The performance of DDR4 interface cannot exceed 1333 Mbps.

The performance Transceiver protocols cannot exceed 10.3125 Gbps.

Rev: 2026.1

The online versions of the documents are provided as a courtesy. Verify all content and data in the device’s PDF documentation found on the device product page.