Jump to main content

##

# 1 MPLAB® Harmony 3 I2C Bootloader Application Examples

MPLAB® Harmony 3 is an extension of the MPLAB® ecosystem for creating embedded firmware solutions for Microchip 32-bit SAM and PIC® microcontroller and microprocessor devices.

This repository contains the MPLAB® Harmony 3 I2C Bootloader application examples

Bootloader Library

Refer to Bootloader Library Help for understanding

- Bootloader framework
- How the Bootloader library works
- Bootloader library configurations
- Bootloader memory layout

Bootloader Examples

The following applications are provided to demonstrate the I2C bootloader

Name | Description
--- | ---
I2C Bootloader | This example application shows how to use the Bootloader Library to bootload an application using I2C protocol
I2C Faile Safe Bootloader | This example application shows how to use the Bootloader Library to bootload an application on device having dual flash bank feature using I2C protocol