Jump to main content

##

# 1.1.5.1.4 Library Interface

SST38 driver library provides the following interfaces:

Functions

Name | Description
--- | ---
DRV_SST38_Initialize | Initializes the SST38 Driver
DRV_SST38_Open | Opens the specified SST38 driver instance and returns a handle to it
DRV_SST38_Close | Closes an opened-instance of the SST38 driver
DRV_SST38_Status | Gets the current status of the SST38 driver module
DRV_SST38_ReadProductId | Reads Manufacturer and Device ID of the SST38 device
DRV_SST38_SectorErase | Erase the sector from the specified block start address
DRV_SST38_ChipErase | Erase entire flash memory
DRV_SST38_Read | Reads n bytes of data from the specified start address of flash memory
DRV_SST38_PageWrite | Writes one page of data starting at the specified address
DRV_SST38_GeometryGet | Returns the geometry of the device
DRV_SST38_TransferStatusGet | Gets the current status of the transfer request

Data types and constants

Name | Type | Description
--- | --- | ---
DRV_SST38_TRANSFER_STATUS | Enum | SST38 Driver Transfer Status
DRV_SST38_GEOMETRY | Struct | Defines the data type for SST38 PROM Geometry details