Jump to main content

##

# DRV_MX25L_ResetFlash Function

## C

    bool DRV_MX25L_ResetFlash(void);

## Summary

Reset the flash device to standby mode.

## Description

This function schedules a blocking operation for resetting the flash device to standby mode. All the volatile bits and settings will be cleared then, which makes the device return to the default status as power on.

## Precondition

The DRV_MX25L_Open() routine must have been called for the specified MX25L driver instance.

## Parameters

Param | Description
--- | ---
handle | A valid open-instance handle, returned from the driver's open routine

## Returns

true - if the reset is successfully completed

false - if Reset-Enable or Reset flash command itself fails

## Example

    if(DRV_MX25L_ResetFlash() == false)
    {
        // Error handling here
    }

## Remarks

This routine will block wait for request to complete.