Jump to main content

##

# DRV_SST38_TransferStatusGet Function

## C

    DRV_SST38_TRANSFER_STATUS DRV_SST38_TransferStatusGet( const DRV_HANDLE handle );

## Summary

Gets the current status of the transfer request.

## Description

This routine gets the current status of the transfer request.

## Preconditions

The DRV_SST38_Open() routine must have been called for the specified SST38 driver instance.

## Parameters

Param | Description
--- | ---
handle | A valid open-instance handle, returned from the driver's open routine

## Returns

DRV_SST38_TRANSFER_ERROR_UNKNOWN - If the handle is invalid.

DRV_SST38_TRANSFER_BUSY - If the current transfer request is still being processed.

DRV_SST38_TRANSFER_COMPLETED - If the transfer request is completed.

## Example

    DRV_HANDLE handle; // Returned from DRV_SST38_Open

    if (DRV_SST38_TransferStatusGet(handle) == DRV_SST38_TRANSFER_COMPLETED)
    {
        // Operation Done
    }

## Remarks

None.