Jump to main content

##

# 1.1.4.4.15 DRV_NAND_FLASH_SkipBlock_BlockRead Function

## C

    bool DRV_NAND_FLASH_SkipBlock_BlockRead(const DRV_HANDLE handle, uint16_t blockNum, uint8_t *data, bool disableBlockCheck)

## Summary

Reads the data of a whole block from NAND Flash.

## Description

This function schedules a blocking operation for reading the data of a whole block from NAND Flash.

## Precondition

The DRV_NAND_FLASH_Open() routine must have been called for the specified NAND FLASH driver instance.

## Parameters

Param | Description
--- | ---
handle | A valid open-instance handle, returned from the driver's open routine
blockNum | Block number to read
data | Pointer to destination data buffer
disableBlockCheck | 0 - Block will be checked as good before reading a given block. 1 - Block will not check before reading a given block.

## Returns

true - If Block read is successfully completed

false - If Block read fails

## Example

    DRV_HANDLE handle; // Returned from DRV_NAND_FLASH_Open
    uint16_t blockNum = 3;
    static uint8_t blockBuffer[262144 + 14336];

    if (DRV_NAND_FLASH_SkipBlock_BlockRead(handle, blockNum, blockBuffer, 0))
    {
        // Block read successfully completed
    }

## Remarks

This routine will block waiting until read request is completed successfully.