Jump to main content

##

# 1.1.8.4.22 DRV_SPI_CS_POLARITY Enum

## C

    typedef enum
    {
        DRV_SPI_CS_POLARITY_ACTIVE_LOW,
        DRV_SPI_CS_POLARITY_ACTIVE_HIGH
    }DRV_SPI_CS_POLARITY;

## Summary

Identifies SPI Chip Select Polarity Options

## Description

This enumeration identifies possible SPI Chip Select Polarity Options.

## Remarks

None.

## Summary

Defines the data required to setup the SPI transfer

## Description

This data type defines the data required to setup the SPI transfer. The data is passed to the DRV_SPI_TransferSetup API to setup the SPI peripheral settings dynamically.

## Remarks

None.