Jump to main content

##

# 1.1.8.4.19 DRV_SPI_CLOCK_PHASE Enum

## C

    typedef enum
    {
        /* Input data is valid on clock trailing edge and
        output data is ready on leading edge */
        DRV_SPI_CLOCK_PHASE_VALID_TRAILING_EDGE,

        /* Input data is valid on clock leading edge and
        output data is ready on trailing edge */
        DRV_SPI_CLOCK_PHASE_VALID_LEADING_EDGE

    }DRV_SPI_CLOCK_PHASE;

## Summary

Identifies SPI Clock Phase Options

## Description

This enumeration identifies possible SPI Clock Phase Options.

## Remarks

None.