Jump to main content

##

# 1.1.7.4.10 DRV_SDSPI_IsAttached Function

## C

    bool DRV_SDSPI_IsAttached
    (
        const DRV_HANDLE handle
    )

## Summary

Returns the physical attach status of the SD Card.

## Description

This function returns the physical attach status of the SD Card.

## Precondition

The DRV_SDSPI_Initialize routine must have been called for the specified SDSPI driver instance.

The DRV_SDSPI_Open routine must have been called to obtain a valid opened device handle.

## Parameters

Param | Description
--- | ---
handle | A valid open-instance handle, returned from the driver's open function

## Returns

true - If the SD Card is attached and initialized by the SDSPI driver.

false - If the handle is invalid

## Example

    bool isSDSPIAttached;

    // mySDSPIHandle is the handle returned by the DRV_SDSPI_Open function.
    isSDSPIAttached = DRV_SDSPI_IsAttached(mySDSPIHandle);

    if (isSDSPIAttached == true)
    {
        // SD Card is attached and initialized by the SDSPI driver.
    }

## Remarks

None.