Jump to main content

##

# 1.1.7.4.19 DRV_SDSPI_COMMAND_STATUS Enum

## C

    typedef enum
    {
        /*Done OK and ready */
        DRV_SDSPI_COMMAND_COMPLETED = SYS_MEDIA_COMMAND_COMPLETED,

        /*Scheduled but not started */
        DRV_SDSPI_COMMAND_QUEUED = SYS_MEDIA_COMMAND_QUEUED,

        /*Currently being in transfer */
        DRV_SDSPI_COMMAND_IN_PROGRESS = SYS_MEDIA_COMMAND_IN_PROGRESS,

        /*Unknown Command */
        DRV_SDSPI_COMMAND_ERROR_UNKNOWN = SYS_MEDIA_COMMAND_UNKNOWN,

    } DRV_SDSPI_COMMAND_STATUS;

## Summary

Identifies the possible events that can result from a request.

## Description

This enumeration identifies the possible status values of a read or write buffer request submitted to the driver.

One of these values is returned by the DRV_SDSPI_CommandStatusGet routine.

## Remarks

Refer sys_media.h for SYS_MEDIA_XXX definitions.