Jump to main content

##

# 1.1.6.4.2 DRV_SDMMC_Status Function

## C

    SYS_STATUS DRV_SDMMC_Status ( SYS_MODULE_OBJ object );

## Summary

Provides the current status of the SD Card driver module.

## Description

This routine provides the current status of the SD Card driver module.

## Precondition

Function DRV_SDMMC_Initialize must have been called before calling this function

## Parameters

Param | Description
--- | ---
object | Driver object handle, returned from the DRV_SDMMC_Initialize routine

## Returns

SYS_STATUS_READY - Indicates that the driver is busy with a previous system level operation and cannot start another Note Any value greater than SYS_STATUS_READY is also a normal running state in which the driver is ready to accept new operations.

SYS_STATUS_UNINITIALIZED - Driver is not initialized.

## Example

    SYS_MODULE_OBJ object; // Returned from DRV_SDMMC_Initialize
    SYS_STATUS status;

    status = DRV_SDMMC_Status(object);

    if (status == SYS_STATUS_READY)
    {
        // Driver is initialized and ready to accept requests
    }

## Remarks

None.