Jump to main content

##

# 1.2.6.9 SYS_DMA_SOURCE_ADDRESSING_MODE Enum

## C

    typedef enum
    {
        /* Source address is always fixed */
        SYS_DMA_SOURCE_ADDRESSING_MODE_FIXED,

        /* Source address is incremented after every transfer */
        SYS_DMA_SOURCE_ADDRESSING_MODE_INCREMENTED,

        /* Used when Addressing mode is not supported */
        SYS_DMA_SOURCE_ADDRESSING_MODE_NONE = -1

    }SYS_DMA_SOURCE_ADDRESSING_MODE;

## Summary

Enumeration of possible DMA source addressing modes.

## Description

This data type provides an enumeration of all possible DMA source addressing modes.

## Remarks

Some of the enum elements may not be applicable for particular device, check MCC generated code before using them.