Jump to main content

##

# 1.1.8.4.21 DRV_SPI_DATA_BITS Enum

## C

    typedef enum
    {
        DRV_SPI_DATA_BITS_8,
        DRV_SPI_DATA_BITS_9,
        DRV_SPI_DATA_BITS_10,
        DRV_SPI_DATA_BITS_11,
        DRV_SPI_DATA_BITS_12,
        DRV_SPI_DATA_BITS_13,
        DRV_SPI_DATA_BITS_14,
        DRV_SPI_DATA_BITS_15,
        DRV_SPI_DATA_BITS_16

    }DRV_SPI_DATA_BITS;

## Summary

Identifies SPI bits per transfer

## Description

This enumeration identifies number of bits per SPI transfer.

## Remarks

For 9 to 15bit modes, data should be right aligned in the 16 bit memory location.