Jump to main content

##

# 1.1.2.4.2 DRV_I2C_Status Function

## C

    SYS_STATUS DRV_I2C_Status( const SYS_MODULE_OBJ object)

## Summary

Gets the current status of the I2C driver module.

## Description

This routine provides the current status of the I2C driver module.

## Precondition

Function DRV_I2C_Initialize should have been called before calling this function.

## Parameters

Param | Description
--- | ---
object | Driver object handle, returned from the DRV_I2C_Initialize routine

## Returns

SYS_STATUS_READY - Initialization has succeeded and the I2C is ready for additional operations.

SYS_STATUS_UNINITIALIZED - Indicates that the driver is not initialized.

## Example

    SYS_MODULE_OBJ object; // Returned from DRV_I2C_Initialize
    SYS_STATUS i2cStatus;

    i2cStatus = DRV_I2C_Status(object);

    if (i2cStatus == SYS_STATUS_READY)
    {
        // This means the driver can be opened using the
        // DRV_I2C_Open() function.
    }

## Remarks

A driver can be opened only when its status is SYS_STATUS_READY.