Jump to main content

##

# 1.1.5.2 SST39 PROM Driver

This driver provides the blocking functions to read, write and erase SST39VF040 PROM memory. The driver uses the peripheral library below to interface with the SST39VF040 memory.

- HEMC Peripheral Library

  - Supports Hardened Static Memory Controller (HSMC).

Key Features:

- Supports single instance of the SST39VF040 and single client to the driver

- Supports Block Erase Operations

- Supports Page/Block Write Operations

- The library can be used in both Bare-Metal and RTOS environments