Jump to main content

##

# 1.3.1.4.5 EMU_EEPROM_PageBufferCommit Function

## C

    EMU_EEPROM_STATUS EMU_EEPROM_PageBufferCommit(void)

## Summary

Commits any cached data to physical non-volatile memory

## Description

Commits the internal SRAM caches to physical non-volatile memory, to ensure that any outstanding cached data is preserved. This function should be called prior to a system reset or shutdown to prevent data loss.

## Precondition

Function EMU_EEPROM_Initialize should have been called before calling this function.

## Parameters

None

## Returns

EMU_EEPROM_STATUS - Enum of type EMU_EEPROM_STATUS. Status code indicating the status of the operation.

## Example

    EMU_EEPROM_PageBufferCommit();

## Remarks

None