Jump to main content

##

# 1.1.9 USART Driver

The USART driver provides application ready routines to read and write data from/to the USART peripheral.

Key Features of USART Driver:

- Supports multi-instance and multi-client mode

- Provides data transfer events

- It works in both Asynchronous and Synchronous modes of operation.

- Features thread-safe functions for use in RTOS applications

- Supports DMA transfers