Jump to main content

##

# 2.2.4.59 USB_DEVICE_RESULT Enumeration

## C

    typedef enum {
      USB_DEVICE_RESULT_ERROR_TRANSFER_QUEUE_FULL,
      USB_DEVICE_RESULT_OK,
      USB_DEVICE_RESULT_ERROR_ENDPOINT_NOT_CONFIGURED,
      USB_DEVICE_RESULT_ERROR_ENDPOINT_INVALID,
      USB_DEVICE_RESULT_ERROR_PARAMETER_INVALID,
      USB_DEVICE_RESULT_ERROR_DEVICE_HANDLE_INVALID,
      USB_DEVICE_RESULT_ERROR_ENDPOINT_HALTED,
      USB_DEVICE_RESULT_ERROR_TERMINATED_BY_HOST,
      USB_DEVICE_RESULT_ERROR
    } USB_DEVICE_RESULT;

## Summary

USB Device Result Enumeration

This enumeration lists the possible USB Device Endpoint operation results. These values are returned by USB Device Endpoint functions.

## Members

Members | Description
USB_DEVICE_RESULT_ERROR_TRANSFER_QUEUE_FULL | Queue is full
USB_DEVICE_RESULT_OK | No Error
USB_DEVICE_RESULT_ERROR_ENDPOINT_NOT_CONFIGURED | Endpoint not configured
USB_DEVICE_RESULT_ERROR_ENDPOINT_INVALID | Endpoint not provisioned in the system
USB_DEVICE_RESULT_ERROR_PARAMETER_INVALID | One or more parameter/s of the function is invalid
USB_DEVICE_RESULT_ERROR_DEVICE_HANDLE_INVALID | Device Handle passed to the function is invalid
USB_DEVICE_RESULT_ERROR_ENDPOINT_HALTED | Transfer terminated because host halted the endpoint
USB_DEVICE_RESULT_ERROR_TERMINATED_BY_HOST | Transfer terminated by host because of a stall clear
USB_DEVICE_RESULT_ERROR | An unspecified error has occurred

## Remarks

None.