Jump to main content

##

# 2.9.4.11 USB_DEVICE_PRINTER_PORT_STATUS Structure

## C

    typedef struct {
      uint8_t errorStatus;
      uint8_t selectStatus;
      uint8_t paperEmptyStatus;
    } USB_DEVICE_PRINTER_PORT_STATUS;

## Summary

USB device Printer Port Status.

This structure defines the Printer status.

## Members

Members | Description
uint8_t errorStatus; | 1 = No Error, 0 = Error
uint8_t selectStatus; | 1 = Selected, 0 = Not Selected
uint8_t paperEmptyStatus; | 1 = Paper Empty, 0 = Paper Not Empty

## Remarks

None.