Jump to main content

##

# 2.3.4.30 USB_DEVICE_AUDIO_EVENT_DATA_STATUS_SEND_COMPLETE Structure

## C

    typedef struct {
      USB_DEVICE_AUDIO_TRANSFER_HANDLE handle;
      USB_DEVICE_AUDIO_RESULT status;
    } USB_DEVICE_AUDIO_EVENT_DATA_STATUS_SEND_COMPLETE;

## Summary

USB Device Audio Function Driver Status Send Complete Event Data.

This data type defines the data structure returned by the driver along with USB_DEVICE_AUDIO_EVENT_STATUS_SEND_COMPLETE event.

## Members

Members | Description
USB_DEVICE_AUDIO_TRANSFER_HANDLE handle; | Transfer handle associated with Status Send request
USB_DEVICE_AUDIO_RESULT status; | Completion status of the transfer

## Remarks

None.