Jump to main content

##

# 3.3.4.56 USB_HOST_AUDIO_V1_STREAM_EVENT_INTERFACE_SET_COMPLETE_DATA Structure

## C

    typedef struct {
      USB_HOST_AUDIO_V1_REQUEST_HANDLE requestHandle;
      USB_HOST_AUDIO_V1_RESULT requestStatus;
    } USB_HOST_AUDIO_V1_STREAM_EVENT_INTERFACE_SET_COMPLETE_DATA, USB_HOST_AUDIO_V1_STREAM_EVENT_SAMPLING_RATE_SET_COMPLETE_DATA, USB_HOST_AUDIO_V1_STREAM_EVENT_SAMPLING_RATE_GET_COMPLETE_DATA;

## Summary

USB Host Audio v1.0 Class Stream Control Event Data.

This data type defines the data structure returned by the Audio V1.0 stream in conjunction with the following events:

- USB_HOST_AUDIO_V1_STREAM_EVENT_INTERFACE_SET_COMPLETE
- USB_HOST_AUDIO_V1_STREAM_EVENT_SAMPLING_FREQUENCY_SET_COMPLETE
- USB_HOST_AUDIO_V1_STREAM_EVENT_SAMPLING_FREQUENCY_GET_COMPLETE

## Members

Members | Description
USB_HOST_AUDIO_V1_REQUEST_HANDLE requestHandle; | Transfer handle of this transfer
USB_HOST_AUDIO_V1_RESULT requestStatus; | Transfer termination status

## Remarks

None.