Jump to main content

##

# 2.3.4.29 USB_DEVICE_AUDIO_EVENT_DATA_INTERFACE_SETTING_CHANGED Structure

## C

    typedef struct {
      uint8_t interfaceNumber;
      uint8_t interfaceAlternateSetting;
    } USB_DEVICE_AUDIO_EVENT_DATA_INTERFACE_SETTING_CHANGED;

## Summary

USB Device Audio Function Driver Alternate Interface Setting Event Data.

This data type defines the data structure returned by the driver along with USB_DEVICE_AUDIO_EVENT_DATA_INTERFACE_SETTING_CHANGED.

## Members

Members | Description
uint8_t interfaceNumber; | Interface number of the interface who setting is to be changed
uint8_t interfaceAlternateSetting; | Alternate setting number

## Remarks

None.