Jump to main content

##

# 3.7.4.5 USB_HOST_MSD_TRANSFER_DIRECTION Enumeration

## C

    typedef enum {
      USB_HOST_MSD_TRANSFER_DIRECTION_HOST_TO_DEVICE = 0x00,
      USB_HOST_MSD_TRANSFER_DIRECTION_DEVICE_TO_HOST = 0x80
    } USB_HOST_MSD_TRANSFER_DIRECTION;

## Summary

USB HOST Transfer Direction

This enumeration specifies the direction of the data stage.

## Members

Members | Description
USB_HOST_MSD_TRANSFER_DIRECTION_HOST_TO_DEVICE = 0x00 | Data moves from host to device
USB_HOST_MSD_TRANSFER_DIRECTION_DEVICE_TO_HOST = 0x80 | Data moves from device to host

## Remarks

None.