Jump to main content

##

# 2.2.4.46 USB_DEVICE_CLIENT_STATUS Enumeration

## C

    typedef enum {
      USB_DEVICE_CLIENT_STATUS_CLOSED,
      USB_DEVICE_CLIENT_STATUS_READY
    } USB_DEVICE_CLIENT_STATUS;

## Summary

USB Device Layer Client Status

This enumeration defines the possible status of the USB Device Layer Client. It is returned by the USB_DEVICE_ClientStatusGet function.

## Members

Members | Description
USB_DEVICE_CLIENT_STATUS_CLOSED | Client is closed or the specified handle is invalid
USB_DEVICE_CLIENT_STATUS_READY | Client is ready

## Remarks

None.