Jump to main content

##

# 3.4.4.17 USB_HOST_CDC_EVENT_ACM_SET_CONTROL_LINE_STATE_COMPLETE_DATA Structure

## C

    typedef struct {
      USB_HOST_CDC_REQUEST_HANDLE requestHandle;
      USB_HOST_CDC_RESULT result;
      size_t length;
    } USB_HOST_CDC_EVENT_ACM_GET_LINE_CODING_COMPLETE_DATA, USB_HOST_CDC_EVENT_ACM_SET_LINE_CODING_COMPLETE_DATA, USB_HOST_CDC_EVENT_ACM_SET_CONTROL_LINE_STATE_COMPLETE_DATA, USB_HOST_CDC_EVENT_ACM_SEND_BREAK_COMPLETE_DATA;

## Summary

USB Host CDC Client Driver Command Event Data.

This data type defines the data structure returned by the driver along with the following events: USB_HOST_CDC_EVENT_ACM_SET_LINE_CODING_COMPLETE_DATA, USB_HOST_CDC_EVENT_ACM_SEND_BREAK_COMPLETE_DATA, USB_HOST_CDC_EVENT_ACM_GET_LINE_CODING_COMPLETE_DATA, USB_HOST_CDC_EVENT_ACM_SET_CONTROL_LINE_STATE_COMPLETE_DATA.

## Members

Members | Description
USB_HOST_CDC_REQUEST_HANDLE requestHandle; | Request handle of this request
USB_HOST_CDC_RESULT result; | Termination status
size_t length; | Size of the data transferred in the request

## Remarks

None.