Jump to main content

##

# 2.6.4.17 USB_DEVICE_HID_RESULT Enumeration

## C

    typedef enum {
      USB_DEVICE_HID_RESULT_OK,
      USB_DEVICE_HID_RESULT_ERROR_TRANSFER_QUEUE_FULL,
      USB_DEVICE_HID_RESULT_ERROR_INSTANCE_NOT_CONFIGURED,
      USB_DEVICE_HID_RESULT_ERROR_INSTANCE_INVALID,
      USB_DEVICE_HID_RESULT_ERROR_TERMINATED_BY_HOST,
      USB_DEVICE_HID_RESULT_ERROR
    } USB_DEVICE_HID_RESULT;

## Summary

USB Device HID Function Driver USB Device HID Result enumeration.

This enumeration lists the possible USB Device HID Function Driver operation results. These values USB Device HID Library functions.

## Members

Members | Description
USB_DEVICE_HID_RESULT_OK | The operation was successful
USB_DEVICE_HID_RESULT_ERROR_TRANSFER_QUEUE_FULL | The transfer queue is full. No new transfers can be scheduled
USB_DEVICE_HID_RESULT_ERROR_INSTANCE_NOT_CONFIGURED | The specified instance is not configured yet
USB_DEVICE_HID_RESULT_ERROR_INSTANCE_INVALID | The specified instance is not provisioned in the system
USB_DEVICE_HID_RESULT_ERROR_TERMINATED_BY_HOST | Transfer terminated by host because of a stall clear
USB_DEVICE_HID_RESULT_ERROR | General Error

## Remarks

None.