Jump to main content

##

# 2.2.4.58 USB_DEVICE_EVENT_DATA_SYNCH_FRAME Structure

## C

    typedef struct {
      USB_ENDPOINT_ADDRESS endpoint;
    } USB_DEVICE_EVENT_DATA_SYNCH_FRAME;

## Summary

USB Device Synch Frame Event Data type.

This data type defines the type of data that is returned by the Device Layer along with the USB_DEVICE_EVENT_SYNCH_FRAME event.

## Members

Members | Description
USB_ENDPOINT_ADDRESS endpoint; | Endpoint for which the Synch Frame number is requested

## Remarks

None.