Jump to main content

##

# 2.4.5.7 USB_DEVICE_AUDIO_V2_EVENT_DATA_SET_ALTERNATE_INTERFACE Structure

## C

    typedef struct {
      uint8_t interfaceNumber;
      uint8_t interfaceAlternateSetting;
    } USB_DEVICE_AUDIO_V2_EVENT_DATA_SET_ALTERNATE_INTERFACE;

## Summary

USB Device Audio v2.0 Function Driver Alternate Interface Setting Event Data.

This data type defines the data structure returned by the driver along with USB_DEVICE_AUDIO_V2_EVENT_DATA_INTERFACE_SETTING_CHANGED.

## Members

Members | Description
uint8_t interfaceNumber; | Interface number of the interface who setting is to be changed
uint8_t interfaceAlternateSetting; | Alternate setting number

## Remarks

None.