Jump to main content

##

# 2.8.3.2 USB_DEVICE_MSD_LUNS_NUMBER Macro

## C

    #define USB_DEVICE_MSD_LUNS_NUMBER 1

## Summary

Number of LUNs

This constant sets maximum possible number of Logical Unit (LUN) an instance of MSD can support. This value should be atleast 1. In cases where multiple MSD Function Driver instances are required, this constant should be set to the maximum number of LUNs required by any MSD Function Driver instanceThe following figure shows a pictorial representation of the MSD function driver initialization data structure.

## Remarks

None.