Jump to main content

##

# 3.2.3.5 USB_HOST_HUB_TIER_LEVEL Macro

## C

    #define USB_HOST_HUB_TIER_LEVEL

## Summary

USB Host Hub Tier Level

This constant defines the maximum hub tiers to be supported by the USB Host application. This constant is considered only if the USB_HOST_HUB_SUPPORT_ENABLE option in specified. If specified, the value should be atleast 1. This means that one hub should be supported. In a case where another hub will be connected to the hub which is connected to the USB Host, the value should be 2. As per the USB specification the maximum number of non-root hub tiers can be 5. Hence the value of this configuration constant should not exceed 5.

## Remarks

None.