Jump to main content

##

# 2.3.4.22 USB_DEVICE_AUDIO_EVENT_DATA_CONTROL_SET_CUR Type

## C

    typedef USB_AUDIO_CONTROL_INTERFACE_REQUEST USB_DEVICE_AUDIO_EVENT_DATA_CONTROL_SET_CUR;

## Summary

USB Device Audio Function Driver Set and Get request data.

This data type defines the data structure returned by the driver along with the USB_DEVICE_AUDIO_EVENT_CONTROL_SET_XXX, USB_DEVICE_AUDIO_EVENT_ENTITY_SET_MEM, USB_DEVICE_AUDIO_EVENT_CONTROL_GET_XXX and USB_DEVICE_AUDIO_EVENT_ENTITY_GET_MEM events.