Jump to main content

##

# 2.2.3.6 USB_DEVICE_BOS_DESCRIPTOR_SUPPORT_ENABLE Macro

## C

    #define USB_DEVICE_BOS_DESCRIPTOR_SUPPORT_ENABLE

## Summary

Specifying this configuration macro will enable support for BOS request. When the request is received, the device layer will transfer the data pointed to by the BOS Descriptor member of the USB_DEVICE_INIT data structure. If this configuration macro is not specified, request for a BOS descriptor is stalled.

## Remarks

The USB Host will request for a BOS descriptor when the bcdVersion field in the Device Descriptor is greater than 0x0200.