Jump to main content

##

# 3.8.6 mcHalI_InverterPwmDisable

## C

    /* Disable three phase inverter */
    void mcHalI_InverterPwmDisable( void )

## Summary

Disable three phase inverter

## Description

This function deactivates the inverter PWM by disabling the specified PWM peripheral instance. It employs the QSpin GUI-configured peripheral API to carry out this operation.

## Precondition

None.

## Parameters

Param | Description
--- | ---
void | None.

## Returns

None

## Example

    /* Disable three phase inverter */
    mcHalI_InverterPwmDisable();

## Remarks

None.