Jump to main content

##

# 3.3.19.7 tmcFly_Parameters_s Struct

## C

    /* Structure defining the parameters for flying start operation */
    typedef struct
    {
        float32_t dt;                      /* Sample time */
        float32_t detectTime;              /* Flying start detection time */
        float32_t minRpmForFlyingStart;    /* Defines the minimum RPM required for a flying start operation */
        float32_t fadeOutTime;             /* Defines the flying start fade out time */
        float32_t fadeOutBurstTime;        /* Defines the flying start fade out burst time */
        uint16_t pwmPeriodCount;           /* Defines the PWM period count value */
        void * pStatePointer;              /* Pointer to the state structure */
    }tmcFly_Parameters_s;

## Summary

Flying start module parameter structure

## Description

This structure holds the parameters for the flying start module. It includes key time constants, speed thresholds, and other necessary configuration data parameters.

## Remarks

None.