Jump to main content

##

# 3.8.7 mcHalI_EncoderStop

## C

    /* Stop encoder pulses counter of quadarature decoder */
    void mcHalI_EncoderStop( void  )

## Summary

Stops the quadrature decoder peripheral.

## Description

The function stops the quadrature decoding process by invoking the specific API for the quadrature decoder instance.

## Precondition

None.

## Parameters

Param | Description
--- | ---
void | None.

## Returns

None

## Example

    /* Stop encoder pulses counter of qudarature decoder */
    mcHalI_EncoderStop();

## Remarks

None.