Jump to main content

##

# 3.8.5 mcHalI_InverterPwmEnable

## C

    /* Enable three phase inverter */
    void mcHalI_InverterPwmEnable( void )

## Summary

Enable the three phase inverter

## Description

This function activates the inverter PWM by enabling the specified PWM module instance. It utilizes the QSpin GUI-configured peripheral API to execute this operation

## Precondition

None.

## Parameters

Param | Description
--- | ---
void | None.

## Returns

None

## Example

    /* Enable three phase inverter */
    mcHalI_InverterPwmEnable();

## Remarks

None.