Jump to main content

##

# 1.1.5.70 SPW_TCH_CFG_RESTART_IN

    typedef enum
    {
        SPW_TCH_CFG_RESTART_IN_PPS = 0,
        SPW_TCH_CFG_RESTART_IN_EVENT = 1,
        /* Force the compiler to reserve 32-bit memory for enum */
        SPW_TCH_CFG_RESTART_IN_INVALID = 0xFFFFFFFF
    } SPW_TCH_CFG_RESTART_IN;

Summary

Identifies the SPW TCH Configure restart input.

Description

This data type identifies the SPW TCH Configure restart input event.