Jump to main content

##

# 1.2.5.58 SPW_PKTTX_PREV

    typedef enum
    {
        SPW_PKTTX_PREV_NOINFO = 0,
        SPW_PKTTX_PREV_LASTSENDLISTOK,
        SPW_PKTTX_PREV_ABORTEDMEMERR,
        SPW_PKTTX_PREV_ABORTEDNEWSD,
        SPW_PKTTX_PREV_ABORTEDUSERCMD,
        SPW_PKTTX_PREV_ABORTEDTIMEOUT,
        /* Force the compiler to reserve 32-bit memory for enum */
        SPW_PKTTX_PREV_INVALID = 0xFFFFFFFF
    } SPW_PKTTX_PREV;

Summary

Identifies the SPW PKTTX Previous status.

Description

This data type identifies the PKTTX Previous status.