Jump to main content

##

# 1.1.5.31 SPW_ROUTER_TIMEOUT_STATUS

    typedef enum
    {
        SPW_ROUTER_TIMEOUT_STATUS_ADDR_MASK = SPW_ROUTER_TIMEOUT_ADDR_Msk,
        SPW_ROUTER_TIMEOUT_STATUS_LOCKED = SPW_ROUTER_TIMEOUT_LOCKED_Msk,
        /* Force the compiler to reserve 32-bit memory for enum */
        SPW_ROUTER_TIMEOUT_STATUS_INVALID = 0xFFFFFFFF
    } SPW_ROUTER_TIMEOUT_STATUS;

Summary

Identifies the SPW ROUTER Timeout current status

Description

This data type identifies the SPW ROUTER Timeout status