Jump to main content

##

# 2.87.8 POWER_DS_ExtendedSemaphoreDisable Function

## C

void POWER_DS_ExtendedSemaphoreDisable(void);

## Summary

Disables the general purpose register retention in the Deep Sleep mode

## Description

Disables the general purpose register retention in the Deep Sleep mode

## Precondition

None.

## Parameters

None.

## Returns

None.

## Example

POWER_DS_ExtendedSemaphoreDisable()

## Remarks

This function is only available for the devices which has deep sleep controller. MCC will generate this function only for the selected devices accordingly. Check device datasheet for more information.