Jump to main content

##

# 2.61.62 LCDCx_SetVSYNCPulseSetupConfig Function

## C

    // x - Instance of the LCDC peripheral

    void LCDCx_SetVSYNCPulseSetupConfig(bool synchronous)

## Summary

Sets the VSYNC pulse sync with HSYNC pulse edge

## Description

None

## Precondition

None.

## Parameters

Param | Description
--- | ---
synchronous | if true, VSYNC is asserted sync with the HSYNC pulse edge if false, VSYNC is asserted one pclk before the HSYNC pulse

## Returns

None

## Remarks

None