Jump to main content

##

# 2.61.29 LCDCx_SetDisplaySignalSynchronization Function

## C

    // x - Instance of the LCDC peripheral

    void LCDCx_SetDisplaySignalSynchronization(bool synchronous)

## Summary

Sets the sync of the DISP signal with the HYSNC pulse

## Description

None

## Precondition

None.

## Parameters

Param | Description
--- | ---
synchronous | if true, DISP signal is sync w/ the 2nd active edge of HSYNC

## Returns

None

## Remarks

None