Jump to main content

##

# 2.99.55 RTC_TamperSourceGet Function

## C

    TAMPER_CHANNEL RTC_TamperSourceGet( void );

## Summary

Get the Tamper source.

## Description

This function returns the channel number that resulted in Tamper Detection interrupt.

## Precondition

Tamper channels must be configured properly using MCC.

## Parameters

Param | Description
--- | ---
reg | Backup register to be used

## Returns

The Tamper channel over which Tamper was detected.

## Example

    //Get Tamper channel
    uint32_t value = RTC_TamperSourceGet();

## Remarks

This Feature may not be available on all devices. Refer to device Datasheet for more information..