Jump to main content

##

# 2.8.62 CANx_MessageAcceptanceMaskSet Function

## C

    void CANx_MessageAcceptanceMaskSet(CAN_MAILBOX_NUM mailbox, uint32_t id) // x - Instance of the CAN peripheral

## Summary

Set Message acceptance identifier mask in mailbox.

## Precondition

CANx_Initialize must have been called for the associated CAN instance.

## Parameters

Param | Description
--- | ---
mailbox | Mailbox number
id | 11-bit or 29-bit identifier

## Returns

None.

## Example

    CAN0_MessageAcceptanceMaskSet(CAN_MAILBOX_0, 0x111);

## Remarks

None.