Jump to main content

##

# 2.73.35 NVMCTRL_RWWEEPROM_Read Function

## C

    bool NVMCTRL_RWWEEPROM_Read( uint32_t *data, uint32_t length, const uint32_t address)

## Summary

Reads length number of bytes from a given address in Data FLASH memory.

## Description

Reads length number of bytes from a given address in Data FLASH memory into the user buffer.

## Precondition

None

## Parameters

Param | Description
--- | ---
data | pointer to user data buffer
length | Number of bytes to read
address | Data FLASH address to be read from

## Returns

Always returns true.

## Example

    uint8_t buffer[256];
    NVMCTRL_RWWEEPROM_Read( (uint32_t *) buffer, 256, 0x20000);