Jump to main content

##

# 2.89.4 PWMx_OffCountSet Function

## C

    /* x = PWM instance number */

    void PWMx_OffCountSet (uint16_t offCount)

## Summary

Sets the off-time period of the PWM signal

## Description

Sets the off-time period of the PWM signal

## Precondition

None

## Parameters

Param | Description
--- | ---
offCount | off-time period of the PWM signal

## Returns

None

## Example

    PWM0_OffCountSet(1000);

## Remarks

None