Jump to main content

##

# 2.8.53 CANx_InterruptEnable Function

## C

    void CANx_InterruptEnable(CAN_INTERRUPT_MASK interruptMask) // x - Instance of the CAN peripheral

## Summary

Enables CAN Interrupt.

## Precondition

CANx_Initialize must have been called for the associated CAN instance.

## Parameters

Param | Description
--- | ---
interruptMask | Interrupt to be enabled

## Returns

None

## Example

    CAN_INTERRUPT_MASK interruptMask = CAN_INTERRUPT_MB0_MASK;
    CAN0_InterruptEnable(interruptMask);

## Remarks

None.