Jump to main content

##

# 2.82.12 PIT_DelayUs Function

## C

    void PIT_DelayUs(uint32_t us);

## Summary

Delays processing for x microseconds.

## Description

Delays execution by using the PIT timer to determine when given number of microseconds has expired.

## Precondition

PIT is configured and enabled. The PIT interrupt is also enabled.

## Parameters

Param | Description
--- | ---
us | number of microseconds to delay

## Returns

None.