Jump to main content

##

# 2.101.3 RTOSTimer_PeriodSet Function

## C

    void RTOSTimer_PeriodSet(uint32_t period)

## Summary

Sets the time period for the RTOS timer

## Description

Sets the timer pre-load register

## Precondition

RTOSTimer_Initialize() function must have been called first.

## Parameters

Param | Description
--- | ---
period | Timer period value

## Returns

None

## Example

    RTOSTimer_PeriodSet(1000);

## Remarks

None