Jump to main content

##

# 2.102.8 RTT_TimerValueGet Function

## C

    uint32_t RTT_TimerValueGet(void);

## Summary

Returns the current timer value

## Description

This function is used the counter value of RTT. This value can be use to calculate the time elapsed.

## Precondition

None.

## Parameters

None.

## Returns

The current timer count

## Example

    uint32_t frequency = 0;
    uint32_t count = 0;
    uint64_t time_elapsed;

    frequency = RTT_FrequencyGet();
    count = RTT_TimerValueGet();

    time_elapsed = count/frequency;